품 명		SUB WOOFER SPEAKER
모 델		METRIX SUB	제조사	ADAMSON
Technical Specifications
	제품스펙 Frequency Response (±3dB) with Full Range Preset : 40Hz to 160Hz Frequency Range Xover Preset : 35HZ to 110Hz Maximum SPL (Continuous/Peak) : 130.4dB / 136.4dB Drivers : ND=15 S 15" Kevlar Neodymium Driver x 2 (6ohms) Power Handling (AES / Program / Peak) : 500 / 1000 / 2000 Sensitivity(2.83V @ 1m) : 104.5dB Connection : Neutrik Speakon™ NL8 Dimensions (WxHxD) :540 x 620 x 733 mm Wight : t-58.7 / i-53.2kg(no rigging)

(주)사운드솔루션

(주)사운드솔루션

3) SUB WOOFER SPEAKER

1. 개  요

전기신호를 음파로 변환시키는 장치

2. 기능 및 특성

컨버터블 카디오이드 서브로서 기존 방식대로 사용할 있을 뿐만 아니라, 짝을 이루어 앞/뒤로 배치하여 카디오이드 성능을 나타낼 수 있어야한다.

15 인치 케블러 네오다이뮴 베이스 드라이버에서 나오는 풍부한 저음으로 Metrix 모델과 최상의 매칭을 이루도록 설계되어야 한다.

리깅 시스템은 스프링 장치가 되어 있어 사용하지 않을 때에는 드러나지 않아야 한다.

- TECHNICAL DATA

Frequency Response (±3dB)

with Full Range Preset	: 40Hz to 160Hz

Frequency Range

Xover Preset	: 35HZ to 110Hz

Maximum SPL (Continuous/Peak)	: 130.4dB / 136.4dB

Drivers	: ND=15 S 15" Kevlar Neodymium Driver x 2 (6ohms)

Power Handling (AES / Program / Peak)            : 500 / 1000 / 2000

Sensitivity(2.83V @ 1m)	: 104.5dB

Connection	: Neutrik Speakon™ NL8

- PHYSICAL DATA

Dimensions (WxHxD)	: 540 x 620 x 733 mm

Wight	: t-58.7 / i-53.2kg(no rigging)

Shap	: Rectangular

Finish	: Black Water Based Bake Enamel

Optional Accessorie	: Black power coated aluminum riging

frame i(t) Steel rigging frame(i), install

adapter plate, Frame Link Plate, Wooden dolly,

Waterproof Soft covers

* METRIX SUB 동등이상품.