품 명		SPEAKER
모 델		METRIX WAVE	제조사	ADAMSON
Technical Specifications
	제품스펙 Frequency Response (±3dB) Full Range Preset / With sub : 95Hz to 18kHz / 35Hz to 18kHz Frequency Range Xover Preset : 125HZ to 18kHz Directivity Horizontal / Vertical : 120° / 15° Sensitivity (2.83v/1m) LMF / HF : 98dB / : 110dB SPL(Continous / Peak) : 126.8 dB / 132.58 dB LF/MF Section (Impedance Ω) : ND8-L 2 8.5" Kevlar Neodymium : Low/Mid-Bass driver (16Ω) HF Section (Impedance Ω) : 3" B&C DE 800 1.4" exit compression driver (16Ω) Power Handling (AES / Program / Peak) L/MF : 250 / 500 / 1000 HF : 110 / 220 / 440 Connection : Neutrik Speakon™ NL8 Dimensions (WxHxD) : 540 x 217 x 420 mm Wight : t-24.2 / i-19.7kg

(주)사운드솔루션

3) SPEAKER

1. 개  요

전기신호를 음파로 변환시키는 장치

2. 기능 및 특성

Adamson Metrix Wave 제품은 수직 15 도의 커버리지를 갖고 있어 Metrix 와 함께 어레이를 이룰 때 각종 다운 필 용도로 사용되기 유용한 모델 입니다.

8.5인치 케블러 네오다이뮴 드라이버와 1.5인치 컴프레션 드라이버에 특허 받은 아담슨 웨이브 쉐이핑 체임버가 장착되어 명료하면서도 맑은 하이 사운드와 풍성하면서 부드러운 미드 레인지가 맞물린 아담슨 만의 독특한 사운드가 재생되어야 한다.

수직 15도, 수평 120도의 지향각을 가져야 하며 각 엔클로져 간 간격은 내장된 AIR 리깅 시스템의 6개로 구분된 리깅 각도에 맞춰 조정하실 수 있어야 한다.

3. 사  양

- TECHNICAL DATA

Frequency Response (±3dB)

Full Range Preset / With sub	: 95Hz to 18kHz / 35Hz to 18kHz

Frequency Range

Xover Preset	: 125HZ to 18kHz

Directivity

Horizontal / Vertical	: 120° / 5°

Sensitivity (2.83v/1m)

LMF / HF	: 98dB / : 110dB

SPL(Continous / Peak)	: 126.8 dB / 132.58 dB

LF/MF Section (Impedance Ω)	: ND8-L 2 8.5" Kevlar Neodymium

: Low/Mid-Bass driver (16Ω)

HF Section (Impedance Ω)	: 3" B&C DE 800 1.4" exit compression driver (16Ω)

Power Handling (AES / Program / Peak)

L/MF	: 250 / 500 / 1000

HF	: 110 / 220 / 440

Connection	: Neutrik Speakon™ NL8

- PHYSICAL DATA

Dimensions (WxHxD)	: 540 x 262 x 420 mm

Wight	: t-24kg / i-19.5kg

Shap	: 15° Trapezoid

Finish	: Black Water Based Bake Enamel

Optional Accessorie	: Black aluminum (t) / steel(i) rigging fram

Rigging	: AIR™ / EIR™

Protective Grille	: 16 Gauge Cold Steel

Cabinet Construction	: Rugged 11 ply Baltic Birch

* METRIX WAVE 동등이상품.

(주)사운드솔루션