품 명		SPEAKER
모 델		SPEKTRIX SUB	제조사	ADAMSON
Technical Specifications
	제품스펙 Frequency Response (±3dB) Full Range Preset : 40Hz to 160Hz Frequency Range Xover Preset : 35HZ to 110Hz Maximum SPL (Continuous) : 132dB Directivity (HxV) : Convertible to Cardioid LF Section : Two adamson Adamson18 AW 2 x 18" : Low Frequency Driver Power Handling (AES / Program / Peak) LF : 600 / 1200 / 2400 Nominal impedance : 4ohms Sensitivity(2.83V @ 1m) : 105.8dB Connection : Neutrik Speakon™ NL8(2 front, 2near) Dimensions (WxHxD) : 640 x 585 x 840 mm Wight : 77kg

(주)사운드솔루션

3) SPEAKER

1. 개  요

전기신호를 음파로 변환시키는 장치

2. 기능 및 특성

SpekTrix 라인 어레이의 서브로 출시된 SpekTrix Sub는 아담슨 최초로 Convertible Cardioid Technology가 실용화한 모델이다.

기존의 방식처럼 모두 동일한 방향으로 향하게 설치해 사용할 수 있을 뿐만 아니라 전면과 후면을 교차한 한 쌍으로 설치하면 진정한 Cardioid 성능을 발휘할 수 있어야 한다.

드라이버는 캐블러 재질로 된 AW18를 2개 장착하여 강력한 성능을 자랑하며, 캐비닛 역시 저음의 공명을 최소화하고 효율은 최대화되도록 설계되어야 한다.

4세트로 구성된 알루미늄 리깅 하드웨어에는 사용하지 않을 때 돌출되지 않도록 스프링 장치가 있으며, 전후면에 각각 2개씩 총 4개의 NL8 커넥터가 있어, 소리의 지향 방향과 상관없이 케이블 연결이 손쉬워야 한다.

- TECHNICAL DATA

Frequency Response (±3dB)

Full Range Preset	: 40Hz to 160Hz

Frequency Range

Xover Preset	: 35HZ to 110Hz

Maximum SPL (Continuous)	: 132dB

Directivity (HxV)	: Convertible to Cardioid

LF Section	: Two adamson Adamson18 AW 2 x 18"

: Low Frequency Driver

Power Handling (AES / Program / Peak)

LF	: 600 / 1200 / 2400

Nominal impedance	: 4ohms

Sensitivity(2.83V @ 1m)	: 105.8dB

Connection	: Neutrik Speakon™ NL8(2 front, 2near)

- PHYSICAL DATA

Dimensions (WxHxD)	: 640 x 585 x 840 mm

Wight	: 77kg

Shap	: Rectangular

Finish	: Black Water Based Bake Enamel

Flying Point	: Four sets of captured rigging: springloaded

: precision machined aluminum

Protective grille	: 14 Gauge cold steel

Cabinet Construction	: Rugged 15-ply Baltic Birch, internally braced

Accessories	: Aluminum Dolly Board

Optional Accessories	: Speck Trix Aluminum Rigging Frame

* SPEKTRIX SUB 동등이상품.