품 명		SPEAKER
모 델		SPEKTRIX WAVE	제조사	ADAMSON
Technical Specifications
	제품스펙 Frequency Response (±3dB) Full Range Preset / with sub : 80Hz to 18kHz / 35Hz to 18kHz Frequency Range Xover Preset : 110HZ to 18kHz Maximum SPL (Continuous) Preset Xover mode : 130.1dB / 136.1dB Preset Full Range : 129.8dB / 135.8dB Maximum SPL (Peak) Preset Xover mode : 136.1dB Preset Full range : 135.8dB Directivity Horizontal / Verical (per elment) : 120 degrees / 15 degrees Sensitivity (2.83v/1m) LF : 94.5dB / 80Hz to 250Hz MF : 99dB / 250Hz to 900Hz HF : 112dB / 900Hz to 18kHz LF Section (Impedance Ω) : ND8-L 8.5" Kevlar Neodymium Mid-Bass driver (8Ω) MF Section (Impedance Ω) : ND8-L 8.5" Kevlar Neodymium Mid-Range driver (8Ω) HF Section (Impedance Ω) : B&C DE 900 1.5" compression driver (8Ω) Power Handling (AES / Program / Peak) LF : 250 / 500 / 1000 MF : 250 / 500 / 1000 HF : 80 / 160 / 320 Connection : Neutrik Speakon™ NL8 Dimensions (WxHxD) : 710 x 220 x 480 mm Wight : 29.03kg

(주)사운드솔루션

3) SPEAKER

1. 개  요

전기신호를 음파로 변환시키는 장치

2. 기능 및 특성

SpekTrix 시리즈를 더욱 효율적으로 사용할 수 있도록 탄생한 SpekTrix Wave는 캐비닛이 15도의 각도를 갖고 있어 다운 필이나 발코니가 많은 극장 같은 수직 커버리지가 커야 할 경우에 유용한 제품이다.

커버리지 패턴은 H120 x V15이며, SpekTrix와 마찬가지로 curved iso-phase wave front를 만들어 내야 한다.

회전 원판 리깅 시스템이 적용되어 모든 리깅 장치가 드러나지 않으며 혼자서도 손쉽게 어레이 작업을 할 수 있어야 한다.

사다리꼴의 캐비닛은 이중으로 흑색 반점 코팅 처리가 된 5/8” 발트해산 자작나무로 만들어 가벼워야 한다. (약28킬로그램)

- TECHNICAL DATA

Frequency Response (±3dB)

Full Range Preset / with sub	: 80Hz to 18kHz / 35Hz to 18kHz

Frequency Range

Xover Preset	: 110HZ to 18kHz

Maximum SPL (Continuous)

Preset Xover mode	: 130.1dB / 136.1dB

Preset Full Range	: 129.8dB / 135.8dB

Maximum SPL (Peak)

Preset Xover mode	: 136.1dB

Preset Full range	: 135.8dB

Directivity Horizontal / Verical (per elment)  : 120 degrees / 15 degrees

Sensitivity (2.83v/1m)

LF	: 94.5dB / 80Hz to 250Hz

MF	: 99dB / 250Hz to 900Hz

HF	: 112dB / 900Hz to 18kHz

LF Section (Impedance Ω)	: ND8-L 8.5" Kevlar Neodymium Mid-Bass driver (8Ω)

MF Section (Impedance Ω)	: ND8-L  8.5" Kevlar Neodymium Mid-Range driver (8Ω)

HF Section (Impedance Ω)	: B&C DE 900 1.5" compression driver (8Ω)

Power Handling (AES / Program / Peak)

LF	: 250 / 500 / 1000

MF	: 250 / 500 / 1000

HF	: 80 / 160 / 320

Connection	: Neutrik Speakon™ NL8

- PHYSICAL DATA

Dimensions (WxHxD)	: 710 x 264 x 480 mm

Wight	: 29.03kg

Shap	: 15° Trapezoid

Finish	: Black Water Based Bake Enamel

Optional Accessorie	: Aluminum rigging frame

Rigging	: AIR™ Revolving Disk Rigging with 3 precise	rigging angles

Protective Grille	: 16 Gauge cold Steel

Cabinet Construction	: Rugged 11ply Baltic Birch

* SPEKTRIX WAVE 동등이상품.