품 명		SUB SPEAKER
모 델		T21SUB	제조사	ADAMSON
Technical Specifications
	제품스펙 Frequency Response (-10dB) single unit : 36Hz to 193Hz Full Range Preset with Preset Y18(Y10) : 30Hz to 70Hz Maximum SPL Continuous with Preset : 140.5dB Peak with Preset : 146.5dB Loudspeakers : 2 x SD-21 21" Kevlar Neodymium Power Handling (AES / Program / Peak) : (300Hz to 300Hz) 1500 / 3000 / 6000 Nominal Impedance(Ohms) : 2x2 Ohms Sensitivity(1m, half space) : 2.83V / 115.6dB / 25Hz to 100Hz Dimensions (WxHxD) : 1463.8 x 584.2 x 973.1 mm Wight : 140.16kg

(주)사운드솔루션

3) SUB SPEAKER

1. 개  요

전기신호를 음파로 변환시키는 장치

2. 기능 및 특성

강력한 서브 베이스음을 보강하기 위해 탄생한 모델로서 플라잉과 스택 모두 가능하며 새로 개발된 다용도 21인치 케블러 드라이버 (SD-21) 2기를 탑재하고 있어야 한다.

탑재된 SD-21 드라이버에는 코일 어셈블리의 양 끝 균형을 잡아주는 독특한 스파이더 서스펜션이 있어 높은 음압 하에서도 음의 변형을 막아줄 뿐만 아니라 6인치 듀얼 보이스 코일/ 네오다이뮴 마그넷과 조화를 이루어 최고의 출력과 센서티비티를 보장 할 수 있어야 한다.

아담슨에서 제작한 드라이버 가운데 가장 최신의 첨단 기술이 들어간 SD-21 드라이버는 스파이더가 공기를 움직이는 역할을 하여 코일의 열을 식힘으로써 작동 온도를 떨어뜨리고 파워 콤프레션을 높여 극도의 파워 핸들링과 왜곡 없는 사운드를 가능케 해야 한다.

3. 사  양

- TECHNICAL DATA

Frequency  Response (-10dB) single unit         : 36Hz to 193Hz

Full Range Preset with Preset Y18(Y10)	: 30Hz to 70Hz

Maximum SPL

Continuous with Preset	: 140.5dB

Peak with Preset	: 146.5dB

Loudspeakers	: 2 x SD-21 21" Kevlar Neodymium

Power Handling (AES / Program / Peak)	: (300Hz to 300Hz)

1500 / 3000 / 6000

Nominal Impedance(Ohms)	: 2x2 Ohms

Sensitivity(1m, half space)	: 2.83V / 115.6dB / 25Hz to 100Hz

- PHYSICAL DATA

Dimensions (WxHxD)	: 1463.8 x 584.2 x 973.1 mm

Wight	: 140.16kg

Finish	: Black Water Based Bake Enamel

Rigging	: Four sets of captured rigging:

spring-loaded precision machined aluminum

Protective	: 14gauge cold rolled steel

Cbinet Construction	: 5/8" Baltic birch, internally braced

Accessorie	: Aluminum dolly board

Optional Accessorie	: Sub rigging frame, Custom soft - cover

Connectinor	: Neutric Speakon™NL8(see jack plate picture below)

* Y10SUB 동등이상품.