품 명		SPEAKER
모 델		Y18	제조사	ADAMSON
Technical Specifications
	제품스펙 Frequency Response (Hz) Full Range Preset : 40Hz to 18kHz Xover Preset : 70Hz to 18kHz Maximum SPL (continuous) with Preset Xover mode : 138.5dB with Preset Full range : 138 dB Maximum SPL (peak) with Preset Xover mode : 144.5dB with Preset Full range : 144dB Sensitivity (2.83v/1m) LF : 104dB (105dB using 2 units) MF : 110dB (110dB using 2 units) HF : 116dB (116dB using 2 units) Directivity Horizontal : 100° @ -6dB / 90° @ -3dB Vertical : 5° (prolate-spheroidal sound chamber) Vertical : several enclosures - defined by the array LF x 2 : AW18 18” Kevlar Drivers (8Ω) MF x 2 : YX9 9” Kevlar Drivers (8Ω) HF 2 x : 2 x JBL 2451 (8Ω) Power Handling (AES / Program / Peak) LF x 2 : 600 / 1200 / 2400 MF x 2 : 350 / 700 / 1400 HF x 2 : 150 / 300 / 600 Connection : Neutrik Speakon™ NL8 Processing : Settings Available for XTA & LAKEResponse Dimensions (WxHxD) : 1466 x 467 x 623 mm Wight : 122.7kg

(주)사운드솔루션

3) SPEAKER

1. 개  요

전기신호를 음파로 변환시키는 장치

2. 기능 및 특성

18인치 저음 드라이버 2개와 9인치 중음/1.5인치 고음 드라이버가 함께 동축으로 장착된 중고음 드라이버 모듈 2기를 장착한 가장 강력한 라인 어레이 모델이어야 한다.

Y18은 중고음 드라이브 모듈과 더불어 캐비닛 사이의 간격을 없앤 사다리꼴 몸체를 통해 일체형 커브 웨이브프론트 (curved iso-phase wavefront)가 형성됨으로써 mid lobing, comb filtering, time-smear 현상 등이 사라져 어떤 PA 시스템보다도 정확한 컨트롤과 넓은 커버리지(H 100 x V2.5(-3dB))을 제공 하여야 한다.

3. 사  양

- TECHNICAL DATA

Frequency Response (Hz)

Full Range Preset	: 40Hz to 18kHz	　　　　　　　　 Xover Preset	: 70Hz to 18kHz

Maximum SPL (continuous)

with Preset Xover mode	: 138.5dB

with Preset Full range	: 138 dB

Maximum SPL (peak)

with Preset Xover mode	: 144.5dB

with Preset Full range	: 144dB

Sensitivity (2.83v/1m)

LF	: 104dB (105dB using 2 units)

MF	: 110dB (110dB using 2 units)

HF	: 116dB (116dB using 2 units)

Directivity

Horizontal	　	: 100° @ -6dB / 90° @ -3dB

Vertical	　　　　	: 5° (prolate-spheroidal sound chamber)

Vertical	　　　　	: several enclosures - defined by the array

LF x 2	: AW18 18” Kevlar Drivers (8Ω)

MF x 2	: YX9 9” Kevlar Drivers (8Ω)

HF 2 x	: 2 x JBL 2451 (8Ω)

Power Handling (AES / Program / Peak)

LF x 2	: 600 / 1200 / 2400

MF x 2	: 350 / 700 / 1400

HF x 2	: 150 / 300 / 600

Connection	: Neutrik Speakon™ NL8

Processing	: Settings Available for XTA & LAKEResponse

- PHYSICAL DATA

Dimensions (WxHxD)	: 1466 x 467 x 623 mm

Wight (Dolly)	: 122.7kg (15.9kg)

Finish	: Black Waterbased Bake Enamel

Rigging	: Stainless/Aluminum Side Hinge

Cabinet Construction	: Rugged 11-ply Baltic Birch

Accessories	: Aluminum Dolly

Optional Accessories	: Powdercoated Black Aluminum, Rigging Frame	Waterproof Custom Soft Cover

* Y18 동등이상품.