품 명		SPEAKER
모 델		Y10	제조사	ADAMSON
Technical Specifications
	제품스펙 Frequency Response (Hz) Full Range Preset : 60Hz to 18kHz Xover Preset : 90Hz to 18kHz Maximum SPL (continuous) with Preset Xover mode : 139.6dB(138.5/2 units) with Preset Full range : 133.8dB(138.5/2 units) Maximum SPL (peak) with Preset Xover mode : 139.6dB(138.5/2 units) with Preset Full range : 133.8dB(138.5/2 units) Sensitivity (2.83v/1m) LF : 99dB (105dB using 2 units) MF : 104dB (110dB using 2 units) HF : 112dB (116dB using 2 units) Directivity Horizontal : 100° @ -6dB / 90° @ -3dB Vertical : 5° (prolate-spheroidal sound chamber) Vertical : several enclosures - defined by the array LF Section (Impedance Ω) : 2 x ND10-L 10” Kevlar Neodymium : Low Frequency Drivers (2 x 16Ω) MF Section (Impedance Ω) : YX9 9” Kevlar Driver (8Ω) HF Section (Impedance Ω) : JBL 2451 (8Ω) Power Handling (AES / Program / Peak) LFx2 : 300 / 600 / 1200 x2 MF : 350 / 700 / 1400 HF : 150 / 300 / 600 Connection : Neutrik Speakon™ NL8 Processing : Settings Available for XTA & LAKE Dimensions (WxHxD) : 1086 x 267 x 623 mm Wight : 57.2kg(15.9kg)

(주)사운드솔루션

3) SPEAKER

1. 개  요

전기신호를 음파로 변환시키는 장치

2. 기능 및 특성

9인치 Kevlar 중음 드라이버(YX9)와 1.5인치 고음 드라이버(JBL2451)가 동축에 장착된 드라이브 모듈 1기와 10인치 저음 드라이버 2기를 장착한 서브 콤팩트 3-way 라인 어레이 모델이어야 한다.

고음과 중음에서 curved iso-phase wavefront가 만들어짐으로써 mid lobing, comb filtering, time-smear 현상 등이 실제로 제거되어 far field에서 타의추종을 불허하는 음명료도를 보여주어야 한다.

다른 3-way 라인 어레이의 절반 정도 크기에도 더 높은 SPL 능력을 보여주어 Y10 2기만으로도 동급의 타사 제품 3기 이상의 효과를 내야 한다.

H100 x V5(-3dB), H90 x V5(-6dB)의 커버리지 패턴을 가지며 수직 커버리지는 캐비닛의 수에 따라 변할 수 있어야 한다.

3. 사  양

-TECHNICAL DATA

Frequency Response (Hz)

Full Range Preset	: 60Hz to 18kHz

Xover Preset	: 90Hz to 18kHz

Maximum SPL (continuous)

with Preset Xover mode	: 139.6dB(138.5/2 units)

with Preset Full range	: 133.8dB(138.5/2 units)

Maximum SPL (peak)

with Preset Xover mode	: 139.6dB(138.5/2 units)

with Preset Full range	: 133.8dB(138.5/2 units)

Sensitivity (2.83v/1m)

LF	: 99dB (105dB using 2 units)

MF	: 104dB (110dB using 2 units)

HF	: 112dB (116dB using 2 units)

Directivity

Horizontal	: 100° @ -6dB / 90° @ -3dB

Vertical	: 5° (prolate-spheroidal sound chamber)

Vertical	: several enclosures - defined by the array

LF Section (Impedance Ω)	: 2 x ND10-L 10” Kevlar Neodymium

: Low Frequency Drivers (2 x 16Ω)

MF Section (Impedance Ω)	: YX9 9” Kevlar Driver (8Ω)

HF Section (Impedance Ω)	: JBL 2451 (8Ω)

Power Handling (AES / Program / Peak)

LFx2	: 300 / 600 / 1200 x2

MF	: 350 / 700 / 1400

HF	: 150 / 300 / 600

Connection	: Neutrik Speakon™ NL8

Processing	: Settings Available for XTA & LAKE

-PHYSICAL DATA

Dimensions (WxHxD)	: 1086 x 267 x 623 mm

Wight (얘LLY)	: 57.2kg(15.9kg)

Finish box	: Black Water based Bake Enamel

Rigging	: Stainless/Aluminum Side Hinge

Cabinet Construction	: Rugged 11ply Baltic Birch

Accessories	: Aluminum Dolly

Optional Accessories	: Powdercoated Black Aluminum, Rigging Frame	Waterproof Custom Soft Cover

* Y10 동등이상품.