품 명		POWER AMPLIFIERS
모 델		FP 2400Q	제조사	LAB. GRUPPEN
Technical Specifications
	제품스펙 KEY FEATURES: 2 X 350 watts @ 8 Ω 2 X 380 watts @ 4 Ω 2 X 500 watts @ 2 Ω (Measured just below clip level, with all 4 channels driven) Compact design, 2U high Low weight, 8kg (18 lbs) MLS™ Switch: Lab.gruppen’s unique power matching for different loads NEW FEATURES: Easily accessible dust filters Improved low-end power bandwidth Extruded front panel for increased stability MAX OUTPUT POWER: Per ch. / Bridge per ch 2ohms : 500w / -3) 4ohms : 590w / 1020w 8ohms : 380w / 760w MAX OUTPUT VOLTAGE: 8 ohms load : 54 Vrma Peak voltage, no load : 81 V CURRENT DRAW AT 4 OHMS AND 230V/115V Dimensions(WxHxD) : 483 x 88 x 316mm Weight : 8.6kg

(주)사운드솔루션

5) POWER AMPLIFIERS

1. 개  요

스피커를 울리기 위하여 필요한 전력을 증폭하여 만들어 내는 기기

2. 기능 및 특성

Compact design, 2U high

Low weight, 7.9kg (17 lbs)

MLS™ Switch: Lab.gruppen’s unique power matching for different loads

Easily accessible dust filters

Improved low-end power bandwidth

Extruded front panel for increased stability

3. 사  양

-MAX OUTPUT POWER:

Per ch. / Bridge per ch

2ohms	: 500w / -3)

4ohms	: 590w / 1020w

8ohms	: 380w / 760w

-MAX OUTPUT  VOLTAGE:

8 ohms load	: 54 Vrma

Peak voltage, no load	: 81 V

- Distortion etc.

THD 20Hz-20kHz and 1W to full power	: 0.07%

THD @ 1kHZ and –1dB under clip	: 0.02 %

DIM 30 at –3dB under clip	: 0.008 %

Hum and Noise	: <–107 dB

Channel separation @10kHz	: 70 dB

Output impedance	: 30 mΩ

Slew Rate	: 60 V/µs

- Inputs

Gain	: 32 dB

Impedance	: 20 kohm

Common mode rejection	: 50 dB

- Front Panel

Gain controls	(2) channel A, B, C, D	31 positions detent

Clip Indicator	(2) red LEDs

Output headroom indicators - slow release Protect

(4x2) green LEDs	Fast peak

Temp Indicator	(4) yellow LEDs	80°C at heatsink

VHF indicator	(4) yellow LEDs	>12 kHz at full power or shorted output

On Indicator	(4) green LEDs	DC rail voltage for channel A,B,C and D

- Rear Panel

Input connectors	(4) Neutrik Combo XLR type, 3 pin and 1/4˝ jack

Output connectors	(4) Neutrik 4-pole Speakon® connectors

- Switches:

Clip limiter A and B	: On–Off (switchable)

MLS switch	: 0,-3 dB

Link-switch	: A+B / B+C / C+D

- Power	230 V version	115 V version

Operation voltage	130 V–265 V AC	65 V–135 V AC

Minimum start voltage

175 V	85 V AC

Full output power at 4ohms

200 V–265 V AC	100 V–130 V AC

Peak inrush current (Soft start limited)

5 A	5 A

- Current Draw @ 4ohms

Quiescent power (no load)

1.4 Arms	2.8 Arms

1/8 of full power (–9 dB)

6 Arms	12 Arms

1/3 of full power (–5 dB)

9 Arms	18 Arms

At full power (0 dB) @1 kHz 1% THD

16 Arms	32 Arms

Dimensions (WxHxD)	: 483 x 88 x 316 mm

Weight	: 8.6 kg

* FP2400Q 동등이상품.