품 명		POWER AMPLIFIERS
모 델		FP 2200	제조사	LAB. GRUPPEN
Technical Specifications
	제품스펙 KEY FEATURES: 2 X 350 watts @ 8 Ω 2 X 650 watts @ 4 Ω 2 X 1100 watts @ 2 Ω (Measured just below clip level, with both channels driven) Compact design, 2U high Intercooler® cooling system with front-to-rear airflow NEW FEATURES: Multiple positions gain switch Easily accessible dust filters Link connector with XLR-type connector Bridged mono outputs in one Speakon® connector Extruded front panel for increased stability MAX OUTPUT POWER: Per ch. / Bridge per ch 2ohms : 1100w / -3) 4ohms : 650w / 2200w 8ohms : 350w / 1400w MAX OUTPUT VOLTAGE: 8 ohms load : 53 Vrma Peak voltage, no load : 77 V CURRENT DRAW AT 4 OHMS AND 230V/115V Dimensions(WxHxD) : 483 x 88 x 287mm Weight : 7.9kg

(주)사운드솔루션

5) POWER AMPLIFIERS

1. 개  요

스피커를 울리기 위하여 필요한 전력을 증폭하여 만들어 내는 기기

2. 기능 및 특성

Compact design, 2U high

Low weight, 7.9kg (17 lbs)

Intercooler® cooling system with front-to-rear airflow

Multiple positions gain switch

Easily accessible dust filters

Link connector with XLR-type connector

Bridged mono outputs in one Speakon® connector

Extruded front panel for increased stability

3. 사  양

- MAX OUTPUT POWER

Per ch. / Bridge per ch

2ohms	: 1100w / -3)

4ohms	: 650w / 2200w

8ohms	: 350w / 1400w

-  MAX OUTPUT  VOLTAGE

8 ohms load	: 53 Vrma

Peak voltage, no load	: 77 V

- Distortion etc

THD 20Hz-20kHz and 1W to full power	: 0.03 %

THD @ 1kHZ and –1dB under clip	: 0.006 %

DIM 30 at –3dB under clip	: 0.008 %

Hum and Noise	: <–110 dB

Channel separation @10kHz	: 70 dB

Output impedance	: 38 mΩ

Slew Rate	: 40 V/µs

- Inputs

Gain, selectable [dB]	: 20, 23, 26, 29, 32, 35, 38, 41

Impedance	: 20 kohm

Common mode rejection	: 50 dB

- Front Panel

Gain controls	(2) channel A, B	31 positions detent

Clip Indicator	(2) red LEDs

Output headroom indicators

(10) green LEDs	Fast peak – slow release

Temp Indicator	(2) yellow LEDs	80°C at heatsink

VHF indicator	(2) yellow LEDs	>12 kHz at full power

On Indicator	(2) green LEDs	DC rail voltage for channel A and B

- Rear Panel

Input connectors	(2) Neutrik Combo XLR type, 3 pin and 1/4˝ jack

Link connector	(2) XLR type, 3 pin male

Output connectors	(2) Neutrik 4-pole Speakon® connectors

- Switches

Clip limiter A and B	: On–Off (switchable)

Link-switch	: Ch. A–B

- Power	230 V version	115 V version

Operation voltage	130 V–265 V AC	65 V–135 V AC

Minimum start voltage

175 V	85 V AC

Full output power at 4ohms

180 V–265 V AC	90 V–130 V AC

Peak inrush current (Soft start limited)

5 A	5 A

- Current Draw @ 4ohms

Quiescent power (no load)

0.9 Arms	1.8 Arms

1/8 of full power (–9 dB)

5 Arms	10 Arms

1/3 of full power (–5 dB)

8 Arms	16 Arms

At full power (0 dB) @1 kHz 1% THD

14 Arms	28 Arms

(AFS limited)	(AFS limited)

Dimensions (WxHxD)	: 483 x 88 x 287 mm

Weight	: 7.9 kg

* FP2200 동등이상품.