품 명		POWER AMPLIFIERS
모 델		iP 1150Q	제조사	LAB. GRUPPEN
Technical Specifications
	제품스펙 - KEY FEATURES: 2 x 130 watts @ 8 Ω 2 x 200 watts @ 4 Ω 2 x 270 watts @ 2 Ω (Measured just below clip level, with both channels driven) Compact design: 2U high Intercooler® cooling system with front-to-rear airflow Multiple positions gain switch Easily accessible dust filter Improved low-end power bandwidth Neutrik Combo jack and Phoenix terminal block input connectors Bridged mono outputs in one SpeakOn connector

(주)사운드솔루션

5) POWER AMPLIFIERS

1. 개  요

스피커를 울리기 위하여 필요한 전력을 증폭하여 만들어 내는 기기

2. 기능 및 특성

Compact design: 2U high

Intercooler® cooling system with front-to-rear airflow

Multiple positions gain switch

Easily accessible dust filter

Improved low-end power bandwidth

Neutrik Combo jack and Phoenix terminal block input connectors

Bridged mono outputs in one SpeakOn connector

3. 사  양

Max output power

EIA at 1 kHz and 1 % THD

- 8 Ω per channel : 130 W

- 4 Ω per channel : 200 W

- 2 Ω per channel : 270 W

- 8 Ω bridged : 400 W

- 4 Ω bridged : 540 W

Max output voltage

- 8 ohms load : 32 Vrms

- Peak voltage, : 51 V

Distortion etc.

THD 20 Hz –20 kHz and 1 W to full power : 0.05 %

THD at 1 kHz and 1 dB below clipping : 0.01 %

DIM 30 at 3 dB below clipping : 0.008 %

Hum and noise : < –05 dB

Channel separation at 10 kHz : 70 dB

Output impedance : 30 mΩ

Slew rate : 30 V/μs

Inputs

Gain selectable : 32

Impedance : 20 kΩ

Common mode rejection : 50 dB

Front panel

Gain controls : 31 pos detent

Indicators per channel:

Protect : Yes

Clip : Yes

Signal present : –40 dB

Rear panel

Input connectors : Neutrik Combo

Clip limiters : On/Off, each ch.

Power

Operation voltage, 230V/115V : 130–60V/65–35V

Soft Start : No

Peak inrush current : 70 A

Full output power at 4 ohms, : 230V/115V

Minimum start-up voltage, : 180/95V

230 V or 115 V versions : Yes

Current draw at 4 Ω and 230V/115V

Idle, no load at output : 0.6 Arms

1/8 of full power (-9 dB) : 2.9 Arms

1/3 of full power (-5 dB) : 4.5 Arms

At full power (0 dB) at 1 kHz 1 % THD : 7.9 Arms

Dimensions

Width : 483 mm (19")

Height : 88 mm(3.5")

Depth : 325 mm (12.8")

Weight : 13.3 kg (29 lbs)

* iP 1150Q 동등이상품.