품 명		POWER AMPLIFIERS
모 델		FP 10000Q	제조사	LAB. GRUPPEN
Technical Specifications
	제품스펙 - General Number of channels : 4 Peak total output both channels driven : 10000 w Peak output voltage per channel : 150 v Max. out current per channel : 38 Arms -Max. output power Per ch.(both ch.'s driven)/Bridged per ch. 2 ohms : 2500w / -3) 4 ohms : 2100w / 50000w 8 ohms : 1300w / 4200w 16 ohms : 660w / 2600w - Perfomance with Gain: 35dB and VPL: 150V THD 20Hz - 20kHz for 1W : <0.1% THD at 1kHz and 1dB below clipping : <0.05% Signal To Noise Ratio : >112 dBA Channel separation (Crosstalk) st 1kHz : >70 dB Frequency response (1W into 8ohms) +0/-3dB : 6.8Hz - 3.4kHz Input impedance : 20 kOhm Input Common Mode Rejection, CMR : 45 dB Output impedance @ 100Hz : 56 mOhm Output slew rate into 8ohms : 20 V/microsecond - Voltage Peak Lomiter(VPL), max. peak output VPL, selectable per ch. : 150, 121, 101, 83, 70, 56, 47, 38v VPL, selectable when bridged1) : 300, 242, 202, 166, 140, 112, 94, 76v Voltage Peak Limiter mode (per ch.) : Hard/Soft - Gain and Level Amplifier gain selectable (all channels)1) - rear-panel switches: 23, 26, 29, 32, 35, 38, 41, 44dB Default gain : 35dB Level adjustment (per ch.): Front-panel potentiometer, 21 position detented form-inf to 0 dB - Connectors and Switches Input connectors (per ch.): 3-pin XLR, electronically balanced Output connectors (per ch.) : Neutrix Speakon or Binding posts (must be specifed upon order) Output bridge mode: A+B, C+D Ch'sA and C are signal input source NomadLink® network: On board, 2 x RJ45 EtherCon connectors, IN and OUT Intelligent fans (on/off): Yes, depending on presence of output signal Power on/off and Remote enable on/off: Individual switches in front-panel Cooling: Two fans, front-to-rear airflow, temperature controlled speed - Front-panel indicators common: NomadLink® network ;Power Average Limiter(PAL)2), Power on Per channel Signal present / High-impedance ;-20dB, -15dB, -10dB and -4dB output signal; Voltage Peak Limiter(VPL); Current Peak Limiter(CPL): Very High Frequency(VHF) - Power Operating voltage, 230V/115V nominal4) : 130-265v / 65-135v Minimum power-up voltage, 230V / 113V : 171v / 85v Power Average Limiter (PAL)2) : Yes Soft start / Inrush Current Draw : Yes / max. 5A Mains connector : 230v CE:16A, CEE7; 115v ETL: 30A Twist loc Dimensions (WxHXD) : 483 x 88 x 396 mm Weight : 12 kg Finish: Black painted steel chassis with black painted steel / aluminum front Approvals: CE, ANSI/UL 60065(ETL), CSA C22.2 NO. 60065, FCC

(주)사운드솔루션

5) POWER AMPLIFIERS

1. 개  요

스피커를 울리기 위하여 필요한 전력을 증폭하여 만들어 내는 기기

2. 기능 및 특성

Very high power and channel density – The four-channel FP10000Q delivers a total of 10000 W (4 x 2500 W @ 2 ohms) in only 2U

Four-channel flexibility – Four channels in one cabinet increases efficiency, flexibility and value in powering monitor systems, line arrays, and bi- or tri-amped systems.. Adjacent channels bridgeable for 2- or 3-channel operation

Lab.gruppen sound quality – FP 10000Q amplifiers maintain the impeccable sonic performance standards set by the original FP Series, with the same durability and even greater efficiency

NomadLink® network ready – Monitoring and control of key functions accessible via the intuitive DeviceControl software and the robust, daisy-chained NomadLink® network

Patented Class TD amplifier topology – Road-proven output stage delivers Class B audio quality with Class D efficiency

Regulated Switch Mode Power Supply (R.SMPS) – Output power remains constant even with significant drops in the mains voltage

Efficient cooling system – Unique, lightweight Intercooler® copper cooling system dissipates more heat to allow extended peak output

Adjustable parameters – Selectable Gain, scalable Voltage Peak Limiter (VPL), and bridge-mode operation allow custom configuration for any system or application

XLR input connectors

Heavy-duty binding post or Speakon output connectors

Comprehensive protection and warning – Excessive output current, DC, high temperature, very high frequency (VHF), short circuit, open load, mains fuse protection, and soft start

3. 사  양

- GENERAL

Number of channels	: 4

Peak total output both channels driven	: 10000 w

Peak output voltage per channel	: 150 v

Max. out current per channel	: 38 Arms

- Max. Output Power

Per ch.(both ch.'s driven)/Bridged per ch.

2 ohms	: 2500w / -3)

4 ohms	: 2100w / 5000w

8 ohms	: 1300w / 4200w

16 ohms	: 660w / 2600w

- Perfomance with Gain: 35dB and VPL: 150V

THD 20Hz - 20kHz for 1W	: <0.1%

THD at 1kHz and 1dB below clipping	: <0.05%

Signal To Noise Ratio	: >112 dBA

Channel separation (Crosstalk) st 1kHz	: >70 dB

Frequency response (1W into 8ohms) +0/-3dB

: 6.8Hz - 3.4kHz

Input impedance	: 20 kOhm

Input Common Mode Rejection, CMR	: 45 dB

Output impedance @ 100Hz	: 56 mOhm

Output slew rate into 8ohms	: 20 V/microsecond

- Voltage Peak Lomiter(VPL), max. peak output

VPL, selectable per ch.	: 150, 121, 101, 83, 70, 56, 47, 38v

VPL, selectable when bridged1)	: 300, 242, 202, 166, 140, 112, 94, 76v

Voltage Peak Limiter mode (per ch.)	: Hard/Soft

- Gain and Level

Amplifier gain selectable (all channels)1) - rear-panel switches

: 23, 26, 29, 32, 35, 38, 41, 44dB

Default gain	: 35dB

level adjustment (per ch.)

: Front-panel potentiometer, 21 position detented form-inf to 0 dB

- connectors and Switches

Input connectors (per ch.): 3-pin XLR, electronically balanced

Output connectors (per ch.)	: Neutrix Speakon or Binding posts (must be specifed upon order)

Output bridge mode: A+B, C+D Ch'sA and C are signal input source

NomadLink® network: On board, 2 x RJ45 EtherCon connectors, IN and OUT

Intelligent fans (on/off): Yes, depending on presence of output signal

Power on/off and Remote enable on/off: Individual switches in front-panel

Cooling: Two fans, front-to-rear airflow, temperature controlled speed

- Front-panel indicators

common: NomadLink® network ;Power Average Limiter(PAL)2), Power on

Per channel

Signal present / High-impedance -20dB, -15dB, -10dB and -4dB output signal;

Voltage Peak Limiter(VPL); Current Peak Limiter(CPL): Very High Frequency(VHF)

- Power

Operating voltage, 230V/115V nominal4)	: 130-265v / 65-135v

Minimum power-up voltage, 230V / 113V	: 171v / 85v

Power Average Limiter (PAL)2)	: Yes

Soft start / Inrush Current Draw	: Yes / max. 5A

Mains connector	: 230v CE:16A, CEE7; 115v ETL: 30A Twist lock

Dimensions (WxHXD)	: 483 x 88 x 396 mm

Weight	: 12 kg

Finish: Black painted steel chassis with black painted steel / aluminum front

Approvals: CE, ANSI/UL 60065(ETL), CSA C22.2 NO. 60065, FCC

* FP10000Q 동등이상품.