품 명		ShotGun Microphone
모 델		MCE 86S II	제조사	beyerdynamic
Technical Specifications
	제품스펙 Transducer type Condenser (back electret) Operating principle Pressure gradient Frequency response 50 - 18,000 Hz Polar patter lobe Hypercardioid/lobe Open circuit voltage at 1 kHz (0 dB = 1V/Pa) 30 mV/Pa Nominal impedance 150 Ω Load impedance ≥1kΩ Max. SPL at 1 kHz 128 dB Signal-to-noise ratio rel. to 1 Pa > 61 dB A-weighted equivalent SPL 25 dB Noise voltage < 25 μVs Male connector 3-pin XLR Supply voltage 11 - 52 V phantom or 1.5 V battery (LR6 AA) (switchable) Current consumption 4 mA / 11 mA (battery) Length 310 mm Diameter 25/21 mm Weight without cable 125 g

(주)사운드솔루션

3) ShotGun Microphone

1. 개  요

일반 마이크로폰 보다 강한 지향성을 얻기 위하여 마이크로폰 앞쪽에 통모양의 도파관을 붙여 예리한 지향성을 가진 장치

2. 기능 및 특성

High sensitivity

Excellent off-axis rejection

Rugged yet lightweight design

Non-glare durable polymer coating

Phantom / Battery power 1.5 V

3. 사  양

- 기술사양

Transducer type	: Condenser (back electret)

Operating principle	: Pressure gradient

Frequency response	: 50 - 18,000 Hz

Polar patter	: lobe Hypercardioid/lobe

Open circuit voltage at 1 kHz (0 dB = 1V/Pa)

: 30 mV/Pa

Nominal impedance	: 150 Ω

Load impedance	: ≥1kΩ

Max. SPL at 1 kHz	: 128 dB

Signal-to-noise ratio rel. to 1 Pa	: > 61 dB

A-weighted equivalent SPL	: 25 dB

Noise voltage	: < 25 μVs

Male connector	: 3-pin XLR

Supply voltage	: 11 - 52 V phantom or 1.5 V battery (LR6 AA) (switchable)

Current consumption	: 4 mA / 11 mA (battery)

Length	: 310 mm

Diameter	: 25/21 mm

Weight without cable	: 125 g

* MCE 86S II 동등이상품.