품 명		Microphone
모 델		M 201 TG	제조사	beyerdynamic
Technical Specifications
	제품스펙 Transducer type Dynamic Operating principle Pressure gradient Frequency response 40 - 18,000 Hz Polar pattern Hypercardioid Rear attenuation at 1 kHz > 20 dB at 120° Open circuit voltage at 1 kHz (0 dB = 1 V/Pa) 1.2 mV/Pa = -58 dBV Magnetic field suspension > 18 dB at 50 Hz Nominal impedance 200 Ω Load impedance ≥ 1000 Ω Diaphragm Hostaphan® Case/finish Brass Connector 3-pin XLR male Dimensions Length: 160 mm Shaft diameter: 24 mm Head diameter: 24 mm Weight without cable 220 g

(주)사운드솔루션

3) Microphone

1. 개  요

가청음을 전기적인 에너지 변환기나 센서로 전달하여 소리를 전기 신호로 변환해 주는 장치

2. 기능 및 특성

Hypercardioid polar pattern

Clarity, neutrality and superior intelligibility

Low-mass moving coil transducer

Rugged construction

Integrated hum-buck coil

3. 사  양

- 기술사양

Transducer type	: Dynamic

Operating principle	: Pressure gradient

Frequency response	: 40 - 18,000 Hz

Polar pattern	: Hypercardioid

Rear attenuation at 1 kHz	: > 20 dB at 120°

Open circuit voltage at 1 kHz (0 dB = 1 V/Pa)

: 1.2 mV/Pa = -58 dBV

Magnetic field suspension	: > 18 dB at 50 Hz

Nominal impedance	: 200 Ω

Load impedance	: ≥ 1000 Ω

Diaphragm	: Hostaphan®

Case/finish	: Brass

Connector	: 3-pin XLR male

Dimensions	: Length: 160 mm
Shaft diameter: 24 mm
Head diameter: 24 mm

Weight without cable	: 220 g

* M 201 TG 동등이상품.