품 명		Microphone
모 델		TG-X 930 Ni	제조사	beyerdynamic
Technical Specifications
	제품스펙 Transducer type Condenser Operating principle Pressure gradient Frequency response 20 - 20,000 Hz Polar pattern Cardioid Open circuit voltage at 1 kHz 4 mV/Pa Nominal impedance 60 Ω Load impedance 1000 Ω Max. SPL at 1 kHz 150 dB Signal-to-noise ratio rel. to 1 Pa approx. 64 dB In-phase rejection 50 - 20,000 Hz ≥ 60 dB A-weighted equivalent SPL 20 dB

(주)사운드솔루션

3) Microphone

1. 개  요

가청음을 전기적인 에너지 변환기나 센서로 전달하여 소리를 전기 신호로 변환해 주는 장치

2. 기능 및 특성

High-quality vocals microphone

Very constant cardioid polar pattern

Compensated close-talking effect

Wire mesh basket without foam

Shock mounted microphone transducer and electronics

velour nickel

3. 사  양

- 기술사양

Transducer type	: Condenser

Operating principle	: Pressure gradient

Frequency response	: 20 - 20,000 Hz

Polar pattern	: Cardioid

Open circuit voltage at 1 kHz	: 4 mV/Pa

Nominal impedance	: 60 Ω

Load impedance	: 1000 Ω

Max. SPL at 1 kHz	: 150 dB

Signal-to-noise ratio rel. to 1 Pa	: approx. 64 dB

In-phase rejection 50 - 20,000 Hz	: ≥ 60 dB

A-weighted equivalent SPL	: 20 dB

* TG-X 930 Ni 동등이상품.