품 명		Microphone
모 델		TG-X 80	제조사	beyerdynamic
Technical Specifications
	제품스펙 Transducer type Dynamic Operating principle Pressure gradient Frequency response Close miking : 20 - 18,000 Hz Distant miking : 85 - 18,000 Hz (measured at 1 metre) Polar pattern Hypercardioid Rear attenuation at 1 kHz > 25 dB at 110° Open circuit voltage at 1 kHz (0 dB = 1V/Pa) 3.2 mV/Pa ± 1.5 dB = -50 dBV Magnetic field suppression > 20 dB at 50 Hz Nominal impedance 280 Ω Load impedance ≥ 1000 Ω Diaphragm Hostaphan® Case/finish Die casting, non-glare black mat Connection 3-pin XLR male Dimensions Length: 205 mm Head diameter: 50 mm Weight without cable 345 g

(주)사운드솔루션

3) Microphone

1. 개  요

가청음을 전기적인 에너지 변환기나 센서로 전달하여 소리를 전기 신호로 변환해 주는 장치

2. 기능 및 특성

Hypercardioid polar pattern

Full range frequency response

Studio quality accuracy

Excellent off-axis rejection

Basket designed for optimum performance

Shock absorbing rubber ring

Structure borne noise attenuation

TG-X 81 switched version

3. 사  양

- 기술사양

Transducer type	: Dynamic

Operating principle	: Pressure gradient

Frequency response	: Close miking : 20 - 18,000 Hz
Distant miking : 85 - 18,000 Hz (measured at 1 metre)

Polar pattern	: Hypercardioid

Rear attenuation at 1 kHz	: > 25 dB at 110°

Open circuit voltage at 1 kHz (0 dB = 1V/Pa)

: 3.2 mV/Pa ± 1.5 dB = -50 dBV

Magnetic field suppression	: > 20 dB at 50 Hz

Nominal impedance	: 280 Ω

Load impedance	: ≥ 1000 Ω

Diaphragm	: Hostaphan®

Case/finish	: Die casting, non-glare black mat

Connection	: 3-pin XLR male

Dimensions	: Length: 205 mm
Head diameter: 50 mm

Weight without cable	: 345 g

* TG-X 80 동등이상품.