품 명		Microphone
모 델		OPUS 29S	제조사	beyerdynamic
Technical Specifications
	제품스펙 Transducer type Dynamic Operating principle Pressure gradient Frequency response (Close miking) 50 - 16,000 Hz (Distant miking) 100 - 14,000 Hz (measured at 1 m) Polar pattern Supercardioid Rear attenuation at 1 kHz > 15 dB at 135° Open circuit voltage at 1 kHz 2.4 mV/Pa Nominal impedance 600 Ω Load impedance 1 kΩ Connection 3-pin XLR male Dimensions Length: 182 mm Shaft diameter 24/37 mm Head diameter 52 mm Weight without cable 320 g

(주)사운드솔루션

3) Microphone

1. 개  요

가청음을 전기적인 에너지 변환기나 센서로 전달하여 소리를 전기 신호로 변환해 주는 장치

2. 기능 및 특성

Entry-level microphone for newcomers

For vocal applications tailored frequency response

High SPL capability

With silent On/Off switch for on-stage control

Durable metal construction

Supplied with standard microphone cable (XLR-XLR, 5 m), microphone clamp

and storage bag

3. 사  양

- 기술사양

Transducer type	: Dynamic

Operating principle	: Pressure gradient

Frequency response	: Close miking : 50 - 16,000 Hz
Distant miking : 100 - 14,000 Hz (measured at 1 m)

Polar pattern	: Supercardioid

Rear attenuation at 1 kHz	: > 15 dB at 135°

Open circuit voltage at 1 kHz	: 2.4 mV/Pa

Nominal impedance	: 600 Ω

Load impedance	: 1 kΩ

Connection	: 3-pin XLR male

Dimensions	: Length: 182 mm

Shaft diameter	: 24/37 mm

Head diameter	: 52 mm

Weight without cable	: 320 g

* OPUS 29S 동등이상품.