모델명	PT-DS20KE			제조사	Panasonic
제품 이미지				밝기	20,000 ANSI Lumens
				DLP™chip	DLP™chip × 3
				해상도	1,470,000(1,400×1,050)
				명암비	10,000:1
				램프	465W UHM lamps(×4)
				크기	620×291×800mm (W×H×D)
				무게	43Kg
◆ 상 세 사 양 ◆
DLP™chip		0.95" 대각선 (화면비율4:3) DLP™chip × 3
해상도		1,470,000(1,400×1,050)
램 프		465W UHM lamp(×4) four-lamp system
밝 기		20,000 ANSI Lumens
명암비		10,000:1 (Full On/Off)
주변조도비		90%
스크린 사이즈		1.78 –15.24 m (70–600 in), ET-D75LE50사용 시 1.78 –7.62 m (70–300 in)
렌즈		Optional powered zoom and fixed-focus lenses
스캔 주파수		SDI	SD-SDI	SMPTE ST 259 compliant, [YCBCR 4:2:2 10-bit] 480i, 576i
			HD-SDI	SMPTE ST 292 compliant, [YCBCR 4:2:2 10-bit] 720/50p, 720/60p, 1035/60i, 1080/50i, 1080/60i,1080/25p,1080/24p,1080/24sF,1080/30p
			DUAL-LINK HD-SDI	SMPTE ST 372 compliant, [RGB4:4:412-bit/10-bit]1080/50i,1080/60i,1080/25p,1080/24p,1080/24sF,1080/30p,[X´Y´Z´4:4:412-bit]2,048x1,080/24p,2,048x1,080/24sF
			3G-SDI	SMPTE ST 424 compliant, [YPBPR 4:2:2 10-bit] 1080/50p, 1080/60p, [RGB4:4:412-bit/10-bit]1080/50i,1080/60i,1080/25p,1080/24p,1080/24Sf,1080/30p
		HDMI / DVI-D		480p, 576p, 720/60p, 720/50p, 1080/60i, 1080/50i, 1080/24p, 1080/24sF,1080/25p,1080/30p,1080/60p,1080/50p, VGA(640x480)–WUXGA(1,920x1,200), compatiblewithnon-interlacedsignalsonly,dotclock:25–162MHz
		RGB		fH: 15–100 kHz, fV: 24–120 Hz, dot clock: 20–162 MHz
		YPBPR (YCBCR)		fH:15.7kHz, fV: 60 Hz[480i (525i)] fH:31.50 kHz, fV: 60 Hz [480p (525p)] fH: 15.63 kHz, fV: 50 Hz [576i (625i)] fH: 31.25 kHz, fV: 50 Hz [576p (625p)] fH: 45.00 kHz, fV: 60 Hz [720 (750)/60p fH: 37.50 kHz, fV: 50 Hz [720 (750)/50p fH: 33.75 kHz, fV: 60 Hz [1035/60i] fH: 33.75 kHz, fV: 60 Hz [1080 (1125)/60i fH: 28.13 kHz, fV: 50 Hz [1080 (1125)/50i] fH: 28.13 kHz, fV: 25 Hz [1080/25p] fH: 27.00 kHz, fV: 24 Hz [1080/24p] fH: 27.00 kHz, fV: 48 Hz [1080/24sF] fH: 33.75 kHz, fV: 30 Hz [1080/30p] fH: 56.25 kHz, fV: 50 Hz [1080/50p] fH: 67.50 kHz, fV: 60 Hz [1080/60p]
		VIDEO		fH: 15.75 kHz, fV: 60 Hz [NTSC/NTSC4.43/PAL-M/PAL60], fH: 15.63 kHz, fV: 50 Hz [PAL/PAL-N/SECAM]
터미널		SDI 1 IN		BNC x 1 (3G/HD/SD-SDI)
		SDI 2 IN		BNC x 1 (HD/SD-SDI)
		3DSYNC IN/OUT		BNC x 1 (3D timing signal)
		3D SYNC OUT		BNC x 1 (3D timing signal)
		DVI-IN		DVI-D 24-pin x 1 (DVI 1.0 compliant, compatible with HDCP, compatible with single link only)
		HDMI IN		HDMI 19-pin x 1 (Deep Color, compatible with HDCP)
		RGB1 IN		BNC x 5 (RGB/YPBPR/YCBCR/YC x 1)
		RGB2 IN		D-Sub HD 15-pin (female) x 1 (RGB/YPBPR/YCBCR x 1)
		VIDEO IN		BNC x 1 (composite video)
		SERIAL IN		D-sub 9-pin (female) x 1(RS-232C compliant)
		SERIAL OUT		D-sub 9-pin (male) x 1(RS-232C compliant)
		REMOTE 1 IN		M3 x 1 for wired remote control
		REMOTE 1 OUT		M3 x 1 for link control (for wired remote control)
		REMOTE 2 IN		D-sub 9-pin (female) x 1 for external control (parallel)
		LAN		RJ-45 x 1 (network connection, 10Base-T/100Base-TX, compliant with PJLink™)
키스톤 보정 범위		수직:±40°, 수평:±15°
전원		220-240 V AC 50/60Hz
소비전력		2,300W
크기(W×H×D)		620×291×800mm
무게		43Kg